IPSM-15 EXPORT FUMIGATION

**AAKASH ENTERPRISE** offers a quality range of ISPM-15 Export Fumigation. The range of services offered at our firm are all professional services with international level of quality. Also, the fumigation services we offer are admired by our clients due to their perfect implementation and our reasonable prices.

In this procedure of fumigation. The wooden cases are positioned inside the fumigation concealments. As well it is enclosed with gas tight sheets to make it an air-tight enclosure. Gas monitoring lines to measure gas congestion during exposure are sited in various gas monitoring areas. The fumigation covers are shielded with sand linings. The total cubic area of ​​the enclosure is measured and the obligatory amount of methyl bromide is introduced in that enclosure. Gas monitoring is performed throughout exposure. After 24 hours of exposure the fumigation covers are detached and vacant wooden boxes are ventilated. At last the ISPM 15 marking is marked on wooden packaging.

At **AAKASH ENTERPRISE** we accomplish all checkmarks with prodigious attention such that your products do not get damaged at any rate. We have our own authorized ISPM-15 Heat Treatment service as well as Fumigation Service also. Also, we provide Export Fumigation Certificate along with Fumigation Stamp on the packaging material if the customer demands.

We offer Certified Fumigation Service- ISPM-15 Standard for 40, 20 feet containers, for export wooden boxes, pallets, saddles, crates etc.

**Plagiarism Report and Words Counter**

